OPEN SOURCE DEM sources

Space Shuttle Radar Topography Mission (SRTM) : 30m res for 16m z accuracy

ASTER Global Digital Elevation Model 30m res (but pb with clouds)

JAXA’s Global ALOS 3D World 30m res

Opendem (open-source) 30m res and less

IGN (France) 30m res (sur http://professionnels.ign.fr/mnt)